            SiS PCI Fast Ethernet Adapter Installation
                     for Windows 95 Driver
            ==========================================

driver file:  .\sisnic.sys
INF file:     .\netsis.inf

Install The Driver
------------------

1.  Install the card in the PCI slot and connect the cable to the network;
    turn on the computer and start Windows 95. **HAVE YOUR WINDOWS 95 CD
    ROM AVAILABLE** because you will need to copy some additional system
    files.

2.  When Windows 95 starts, a "New Hardware Found" dialog box appears
    identifying the card as a "PCI Ethernet Controller". Select
    "Driver from disk provided by the hardware manufacturer" then click OK.

    NOTE, if the "New Hardware Found" dialog box does not appear, please
    do the followings

    a. After entering Windows 95, double click "My Computer".
    b. Double click "Control Panel".
    c. Double click "System".
    d. Click the "Device Manager" tab.
    e. Open "Other Devices" (with "?" icon on it).
    f. Select "PCI Ethernet Controller" then click "Remove" button.

       Note, if you do not see any "PCI Ethernet Controller", Windows 95
       fails to detect your adapter. There may be problem with the adapter
       itself or with the system BIOS.

    g. Restart Windows 95 and goto step 2.

3.  Insert the "SiS PCI Fast Ethernet Aapter Drivers Disk" in your floppy
    drive and specify the correct path, i.e. A:\Win95 or B:\Win95,
    then click OK.

4.  Follow the rest screen instructions to complete the installation.

5.  You should restart your computer for the changes to take effect after
    the installation is complete.


Adapter Configuration
---------------------

1. Double click "My Computer".
2. Double click "Control Panel".
3. Double click "Network" icon.
4. Select
   "SiS 0900 PCI Fast Ethernet Adapter" or
   "SiS 7016 PCI Fast Ethernet Adapter"
   then click "Properties..." button.
5. Click "Advanced" tab.
6. Here, you can set the following properties:

   <1>. MediaType

             100BaseTX
             100BaseTX Full_Duplex
             10BaseT Full_Duplex
             10BaseT
             AUTO_CONFIG   ;Default value if not set

7. After setting the properties, you must restart your computer to
   make the changes effective.

---End of File---


