1.   From Windows Me/98SE, open the Control Panel from ˇ°My Computerˇ± followed by the System 
   icon.

2.   Choose the "Device Manager" tab.

3.   Click the "+" in front of " IDE ATA/ATAPI Controllers" hardware type. The driver 
  " SiS 180 IDE Dual Channel " and " SiS 180 IDE/RAID  Controller " should appear.

4.   The path is ChipDrv\SISRaid\RAID304c\win98me
