
          SiS 900/7016 PCI Fast Ethernet Adapter Installation 
                           for NDIS Driver

LAN Manager v2.2
============================================
1. Execute the setup program in the LAN Manager directory.

     Type: >a:\setup

2. Choose "Network Drivers" from the "Configuration" field.
   Press <Enter> to confirm your choice.

3. Choose <Add New Config> and press <Enter> to display a list
   of Network Adapter Drivers.

4. Choose <Other Driver> and press <Enter>.

5. Insert the Driver Diskette into drive A:. Specify the drive 
   location of the diskette and select <OK> to proceed.

6. Select the appropriate Network Adapter Driver from the list.
   Select

        "SiS 900/7016 PCI Fast Ethernet Adapter"

   Select <OK> to confirm your choice.

7. To continue with the remainder of the installation, select a protocol 
   to use with the SIS 900/7016 PCI Fast Ethernet adapter driver.
   Continue with the remaining installation steps for Lan Manager.


Sample Configuration Files
==========================

  CONFIG.SYS File

        LASTDRIVE=Z
        BUFFERS = 35
        FILES = 35
        SHELL=C:\DOS62\COMMAND.COM C:\DOS62 /p /E:1024
        DEVICE=C:\HIMEM.SYS
        ; remark this line
        REM DEVICE=C:\LANMAN.DOS\DRIVERS\DOSUTILS\EMM386.EXE NoEMS 
        DEVICE=C:\DOS62\SETVER.EXE                       
        DOS=HIGH,UMB
        DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /i:C:\LANMAN.DOS
        DEVICE=C:\LANMAN.DOS\DRIVERS\ETHERNET\SIS900\SIS900.DOS

  PROTOCOL.INI File

        [PROTMAN]
         DRIVERNAME = PROTMAN$
         DYNAMIC = YES
         PRIORITY = NETBEUI
        [NETBEUI_XIF]
         Drivername = netbeui$
         SESSIONS = 6
         NCBS = 12
         BINDINGS = "SIS900_NIF"
         LANABASE = 0

        [SIS900_NIF]
        ;----------------------------------------------------------------------
        ; Sample Protocol.ini file for SIS 900 NDIS/2 driver
        ;----------------------------------------------------------------------
          DriverName = SIS900$
       
        ; End of this sample file

  AUTOEXEC.BAT File

        @echo off
        PROMPT $P$G
        PATH=C:\DOS;
        @REM ====== LANMAN 2.2 === DO NOT MODIFY BETWEEN THESE LINES
        @REM=== LANMAN 2.2 ===
        SET PATH=C:\LANMAN.DOS\NETPROG;%PATH%
        NET START WORKSTATION
        LOAD NETBEUI
        @REM ====== LANMAN 2.2 === DO NOT MODIFY BETWEEN THESE LINES
        @REM === LANMAN 2.2 ===
